
Notations of vibration feeding devices of  
„TEMP-01 LTD”
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2. Combined feeding with two VDFHD (Left and Right propulsion)

    VDFHD – R.D                       VDFHD – R.L                                              VDFHD – R.L                       VDFHD – R.D.              


3. Technical specifications of VDFHD
     




	Type VDFHD   

         Dimension                        
	VDFHD 170
	VDFHD 310
	VDFHD 420
	VDFHD 480

	А [mm]
	170
	310
	420
	480

	C [mm]*
	230
	450
	650
	750

	B[mm]**
	300
	350
	385
	440

	Mass [kg]***
	9,300
	46,800
	62,000
	134,000


* Dimension C is the maximum one for the corresponding type of VDFHD
** Dimension B is valid for the maximum C dimension
*** The mass of the corresponding type VDFHD is valid for the maximum C dimension
4.    VDFHD– L – 420



   Mass of VDFHD -L-420 – 14 кг. 
5. Power supply 
 The devices operate at 220V/50; 60Hz through voltage, delivered by „TEMP-01 LTD”.Protection degree of the entire configuration – IP-20 .

6. Prices
 The prices are negotiable and depend on:

· The type of VDFHD
· Specificity of the objects oriented (complexity, parameters, dimensions, material, availability of delicate parts, elements and roofing material and etc.)

· Required productiveness (Pcs. /min.)

· Time for autonomous work (the time between two loading of objects)

· Package and delivery terms
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